**PREREQUISITES FOR CI/CD**

1. PUTTY INSTALLATION


Step1: Download the putty installation file from

<http://www.putty.org/>


Step2: Find the IP address/Host Name of the server using the following command.

Command: ip address/ip –a


Step3: Then open Putty.exe file



Step4: Enter the IP address/Hostname of the Server.




Step5: Click on open



Step6: Enter login id and password.

User Name: root

Password:admin@123




2. MTPUTTY INSTALLATION


[MTPuTTY (Multi-Tabbed PuTTY) is a small FREE utility enabling you to wrap unlimited number of PuTTY application in one tabbed GUI interface]


Step1: Download MTPuTTY installation package file from the below link.


<http://ttyplus.com/downloads.html>

Step2: Extract the file downloaded (mtputty.zip) and Click on MTPuTTY\_setup.exe and Click on next.











Step5: Click on Install and Finish.







MTPuTTY is installed.

Step6: Open MTPuTTY icon on the desktop and give the location of the Putty.exe file location.

Step7: Click on Server🡪Add Server



Step8:



Step9: Enter Server name, Protocol, Port number, User name and Password and Click on OK.


Server Name: 192.168.70.52 to 192.168.70.64

Protocol: SSH

Port Number: 22

User Name: root

Password:admin@123



Step10: Click on the Server Name.

